CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.5/conf/instr/spect/uxnmr.info
Date         : Wed Jan  8 15:35:53 2025
Release      : TopSpin 3.6.5
Installed in : /opt/topspin3.6.5
Host         : CZC8508V38
OS           : CentOS Linux release 7.6.1810 (Core) 
CPU          : Intel(R) Xeon(R) W-2123 CPU @ 3.60GHz (8 cores at 1200 MHz with Hyperthreading)
User         : nmrsu (NMR Super User)
System       : Avance III 600 NMR spectrometer
1H-frequency : 600.42 MHz
Description  : Avance III 600
Location     : Dept. of Chemical Physics Weismann Inst. of Sciences  76100 Rehovo Israel
Bruker Order : 10136871
Configured in: CZC8508V38:/opt/topspin3.6.5/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.92
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 3
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/01735 ECL 06.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x4    AW  R  4.4 REC-1  AQS RXAD600 Z102117/816 ECL 04.04
     3   0x34 0xc0   0x1        X  2.2 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x19   0x8    AE  S  2.7 SGU-1  AQS SGU/2 600 Z103081/01658 ECL 02.07 FPGA-Vs=AF
     5   0x25 0x19   0x8    AE  S  2.7 SGU-2  AQS SGU/2 600 Z103081/01659 ECL 02.07 FPGA-Vs=AF
     6   0x26 0x19   0x8    AE  S  2.7 SGU-3  AQS SGU/2 600 Z103081/01660 ECL 02.07 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345096_0429 W1345096/0429 ECL 2:
- TCP/IP address = 149.236.99.91
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ INR: W1345096/0429 ECL 2
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0703 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/00883 ECL 03
BLA_W1345092_0483 W1345092/0483 ECL 1:
- TCP/IP address = 149.236.99.90
- Firmware VS    = 20120627
- Amplifier      = BLAX300 E 6-365MHZ INR: W1345092/0483 ECL 1
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/1717 ECL 2
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/5919 ECL 50
LTRX Z109890/00047 ECL 01.02:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00047 ECL 01.02

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20191111
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00047 ECL 01.02
- Lock: on L-TRX board

Eurotherm VTU: device connected to 149.236.99.92:/dev/tty05

Prodigy Control Unit: PCU - LNP PRODIGY UNIT Z127349/259
- TCP/IP address   = 149.236.99.94

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                PN=Z003462, SN=00694 from 20091005
    Module  2 : XBB19F 2HS
                PN=Z003506, SN=00813 from 20091015
    Module  3 : 13C
                PN=Z003524, SN=00167 from 20030116
    Module  4 : 15N
                PN=Z003530, SN=00089 from 20021128
    Module  5 : 2H
                PN=Z003473, SN=00704 from 20091006



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ BLAX300 E 6-365MHZ INR W1345096/0429 at TCP/IP 149.236.99.91)
SGU1 AUX  output -> input 2 of transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0483 at TCP/IP 149.236.99.90)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ BLAX300 E 6-365MHZ INR W1345096/0429 at TCP/IP 149.236.99.91)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0483 at TCP/IP 149.236.99.90)
SGU3 AUX  output -> input 4 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ BLAX300 E 6-365MHZ INR W1345096/0429 at TCP/IP 149.236.99.91)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAXH2H300/100/150 E 200-600MHZ BLAX300 E 6-365MHZ INR W1345096/0429 at TCP/IP 149.236.99.91:
- amplifier 1H-100W uses blanking 2
- amplifier X-300W uses blanking 1
- amplifier 2H-150W needs no blanking

transmitter 2 = BLAX300 E 6-365MHZ INR W1345092/0483 at TCP/IP 149.236.99.90:
- amplifier X-300W uses blanking 3

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 600 Z109890/00047 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


