20 	 21 	 2 	 1 	 24 	  ! Ne, Nn, Nb, Nm, Np 	 
 2	2	1			! Nd, Ng, Ns                              
1.	0.	1.	1.		! Sx, Kappa, tc, por                              
340.	0.1	20.	! tmax, dt, dto                                                            
1.			! theta                              
0	0	-1	! ipar(2:3), ipar(6)                              
1.e-9	1.e-9	0.	! fpar(1:2), fpar(11)                                                            
1000	1.e-3		! maxit, Ctol                              
--------------------------------------------------------------------------------                              
! comparison to Scheidegger Toolbox run (Brian\ctrw_v3.1\data1_fit_EXP.*)                                                            
! with C(x,0) = 0                                                            
! 0 < x < 1, L = 1, Ne = 20, Ns = 1, Np = 24, uniform grid                                                            
--------------------------------------------------------------------------------                              
! parameters:                              
Ne	! total # of elements                              
Nn	! total # of nodes                              
Nb	! total # of BC faces                              
Nm	! total # of materials                              
Np	! # of Prony terms (not includinp p=0)                              
	!	ADE for Np=0, EXP for Np>0 (the same for all materials!!)                              
Nd	! max elements per node                              
Ng	! max Gauss points in each coordinate                              
Ns	! total # of species                              
                              
! properties:                              
Sx	! cross section area normal to x                              
Kappa	! reaction kinetic coefficient                              
tc	! charachteristic time for the reaction                              
por	! porosity                              
                              
! time:                              
tmax	! time at end of group i                              
dt	! time step of time group i                              
dto	! time step for output of time group i                              
                              
! temporal scheme                              
theta	! implicitness factor (0 - explicit, 0.5 - CN, 1 - fully implicit)                              
                              
! biCGstab input:                              
! ipar(1:3), ipar(5:6), fpar(1:2), fpar(11) - see comments in biCGstab                              
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!                              
! initial setting TEMPORARY, to be done in READIN or INIT                              
	ipar( 1) = 0	! start bCGstab solver                              
	ipar( 2) = 0	! no preconditioning                              
	ipar( 3) = 0	! default stopping criteria                              
	ipar( 4) = ldw	! work array dimension for bCGstab                              
	ipar( 5) = 0	! Krylov subspace dimension (unused for bCGstab)                              
	ipar( 6) =-1	! max. [A]{v} operations (unlimited if <0)                              
	ipar(11) = 0	! initialize FLOP counter                              
	fpar( 1) = tol	! relative tolerance                              
	fpar( 2) = tol	! absolute tolerance                              
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!                              
                              
! implicit BC and source convergence parameters                              
maxit	! max. no. of iterations                              
Ctol	! allowabe max. dif. of C                              
--------------------------------------------------------------------------------                              
formers:                              
--------------------------------------------------------------------------------                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
                              
